Krea 911-11 is a light-weight fabric that requires special handling for use in a Colorado print engine.  It is recommended to queue together several jobs or copies for this material to minimize waste.

-Pause the print queue.  Web from roll Position 2 for Print-Side-In.

-Attach a semi-rigid strip of material at least 54” wide (1375mm) and 20" long (500mm) to the leading edge of the material with tape spanning front and back.  Examples of suitable material would be scraps of thin paper, banner, or vinyl that is not too curled.  Refer to your Operations manual for instructions.

-Bring the material to the platen using the FEED button in the Media menu on the printer.  Apply the tension bar in an unlocked position, following the screen prompts.  This profile is set to "Requires Manual Loading" so the printer will not scan width until the first print.  This allows an opportunity to smooth out any wrinkles from the lead strip.  Smooth wrinkles by moving the media forward and backward from the Output menu.

-Resume the queue when ready.  Try to combine as many jobs as possible before cutting.  Follow the screen prompts when ready to cut.  Feeding to the platen again will require another lead strip.
