Ahlstrom WallStar WL8852300 Non-Woven 300gsm 460-US2501

The attached profile has a LOCKED tension bar enabled because of the material's stiffness.  It may become necessary to feed out a 3 to 4 inches of material before printing the first job after loading as the roll nears the end.  Stiff media can sometimes resist forming a blouse just beyond where a locked tension bar rests and rise off the platen into the cure carriage path.  Feeding extra material will not be necessary after enough blouse has formed.

The tension bar can be disabled when using the take-up reel if you choose to manually help form the blouse. (Not recommended)