Canon Generic FAX Driver Version 10.06 for Microsoft Windows
CANON SOFTWARE LICENSE AGREEMENT
IMPORTANT!
This is a legal agreement ("Agreement") between you and Canon Inc. ("Canon") and governing your use of Canon's software programs including the related manuals or any printed material thereof (the "Software") for certain Canon's copying machines, printers and multifunctional peripherals (the "Products").
READ CAREFULLY AND UNDERSTAND ALL OF THE RIGHTS AND RESTRICTIONS DESCRIBED IN THIS AGREEMENT BEFORE INSTALLING THE SOFTWARE. BY CLICKING THE BUTTON INDICATING YOUR ACCEPTANCE AS STATED BELOW OR INSTALLING THE SOFTWARE, YOU AGREE TO BE BOUND BY THE TERMS AND CONDITIONS OF THIS AGREEMENT. IF YOU DO NOT AGREE TO THE FOLLOWING TERMS AND CONDITIONS OF THIS AGREEMENT, DO NOT USE THE SOFTWARE. NO REFUND WILL BE MADE BECAUSE THE SOFTWARE WAS PROVIDED TO YOU AT NO CHARGE.
1. GRANT OF LICENSE
Canon grants you a personal, limited and non-exclusive license to use ("use" as used herein shall include storing, loading, installing, accessing, executing or displaying) the Software solely for the use with Products only on computers directly or via network connected to the Products (the "Designated Computer").
You may allow other users of other computers connected to your Designated Computer to use the Software, provided that you must assure that all such users shall abide by the terms of this Agreement and shall be subject to restrictions and obligations borne by you hereunder.
You may make one copy of the Software solely for a back-up purpose.
2. RESTRICTIONS
You shall not use the Software except as expressly granted or permitted herein, and shall not assign, sublicense, sell, rent, lease, loan, convey or transfer to any third party the Software. You shall not alter, translate or convert to another programming language, modify, disassemble, decompile or otherwise reverse engineer the Software and you shall not have any third party to do so.
3. COPYRIGHT NOTICE
You shall not modify, remove or delete any copyright notice of Canon or its licensors contained in the Software, including any copy thereof.
4. OWNERSHIP
Canon and its licensors retain in all respects the title, ownership and intellectual property rights in and to the Software. Except as expressly provided herein, no license or right, express or implied, is hereby conveyed or granted by Canon to you for any intellectual property of Canon and its licensors.
5. EXPORT RESTRICTION
You agree to comply with all export laws and restrictions and regulations of the country involved, and not to export or re-export, directly or indirectly, the Software in violation of any such laws, restrictions and regulations, or without all necessary approvals.
6. NO SUPPORT
NEITHER CANON, CANON'S SUBSIDIARIES OR AFFILIATES, THEIR DISTRIBUTORS, OR DEALERS NOR CANON'S LICENSORS ARE RESPONSIBLE FOR MAINTAINING OR HELPING YOU TO USE THE SOFTWARE. NO UPDATES, FIXES OR SUPPORTS WILL BE MADE AVAILABLE FOR THE SOFTWARE.
7. NO WARRANTY AND DISCLAIMER OF INDEMNITY
[NO WARRANTY] THE SOFTWARE IS PROVIDED "AS IS" WITHOUT WARRANTY OF ANY KIND, EITHER EXPRESSED OR IMPLIED, INCLUDING, BUT NOT LIMITED TO THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE. THE ENTIRE RISK AS TO THE QUALITY AND PERFORMANCE OF THE SOFTWARE IS WITH YOU. SHOULD THE SOFTWARE PROVE DEFECTIVE, YOU ASSUME THE ENTIRE COST OF ALL NECESSARY SERVICING, REPAIR OR CORRECTION. SOME STATES OR LEGAL JURISDICTIONS DO NOT ALLOW THE EXCLUSION OF IMPLIED WARRANTIES, SO THE ABOVE EXCLUSION MAY NOT APPLY TO YOU.
THIS WARRANTY GIVES YOU SPECIFIC LEGAL RIGHTS AND YOU MAY ALSO HAVE OTHER RIGHTS WHICH VARY FROM STATE TO STATE OR JURISDICTION TO JURISDICTION.
NEITHER CANON, CANON'S SUBSIDIARIES OR AFFILIATES, THEIR DISTRIBUTORS, OR DEALERS NOR CANON'S LICENSORS WARRANT THAT THE FUNCTIONS CONTAINED IN THE SOFTWARE WILL MEET YOUR REQUIREMENTS OR THAT THE OPERATION OF THE SOFTWARE WILL BE UNINTERRUPTED OR ERROR FREE.
[NO LIABILITY FOR DAMAGES] IN NO EVENT SHALL EITHER CANON, CANON'S SUBSIDIARIES OR AFFILIATES, THEIR DISTRIBUTORS DEALERS OR CANON'S LICENSORS BE LIABLE FOR ANY DAMAGES WHATSOEVER (INCLUDING WITHOUT LIMITATION, LOSS OF BUSINESS PROFITS, LOSS OF BUSINESS INFORMATION, LOSS OF BUSINESS INTERRUPTION OR OTHER COMPENSATORY, INCIDENTAL OR CONSEQUENTIAL DAMAGES) ARISING OUT OF THE SOFTWARE, USE THEREOF OR INABILITY TO USE THE SOFTWARE EVEN IF EITHER CANON, CANON'S SUBSIDIARIES OR AFFILIATES, THEIR DISTRIBUTORS, DEALERS OR CANON'S LICENSORS HAVE BEEN ADVISED OF THE POSSIBILITY OF SUCH DAMAGES. SOME STATES OR LEGAL JURISDICTIONS DO NOT ALLOW THE LIMITATION OR EXCLUSION OF LIABILITY FOR INCIDENTAL OR CONSEQUENTIAL DAMAGES, OR PERSONAL INJURY OR DEATH RESULTING FROM NEGLIGENCE ON THE PART OF SELLER, SO THE ABOVE LIMITATION OR EXCLUSION MAY NOT APPLY TO YOU.
[RELEASE OF LIABILITY] TO THE FULL EXTENT PERMITTED BY APPLICABLE LAW, YOU HEREBY RELEASE CANON, CANON'S SUBSIDIARIES AND AFFILIATES, THEIR DISTRIBUTORS, DEALERS AND CANON'S LICENSORS FROM ANY AND ALL LIABILITY ARISING FROM OR RELATED TO ALL CLAIMS CONCERNING THE SOFTWARE OR ITS USE.
8. TERM
This Agreement is effective upon your acceptance hereof by clicking the button indicating your acceptance as stated below or installing the Software and remains in effect until terminated. You may terminate this Agreement by destroying the Software including any and all copies thereof.
This Agreement shall also terminate if you fail to comply with any terms hereof. Upon termination of this Agreement, in addition to Canon enforcing its respective legal rights, you must then promptly destroy the Software including any and all copies thereof. Notwithstanding the foregoing, Sections 4, and 7 through 11 shall survive any termination of this Agreement.
9. U.S. GOVERNMENT RESTRICTED RIGHTS NOTICE
The Software is a "commercial item," as that term is defined at 48 C.F.R. 2.101 (October 1995), consisting of "commercial computer software" and "commercial computer software documentation," as such terms are used in 48 C.F.R. 12.212 (September 1995). Consistent with 48 C.F.R. 12.212 and 48 C.F.R. 227.7202-1 through 227.7202-4 (June 1995), all U.S. Government End Users shall acquire the Software with only those rights set forth herein. Manufacturer is Canon Inc./30-2, Shimomaruko 3-chome, Ohta-ku, Tokyo 146-8501, Japan.
10. SEVERABILITY
In the event that any section hereof is declared or found to be illegal by any court or tribunal of competent jurisdiction, such section shall be null and void with respect to the jurisdiction of that court or tribunal and all the remaining provisions hereof shall remain in full force and effect.
11. ACKNOWLEDGEMENT
BY CLICKING THE BUTTON INDICATING YOUR ACCEPTANCE AS STATED BELOW OR INSTALLING THE SOFTWARE, YOU ACKNOWLEDGE THAT YOU HAVE READ THIS AGREEMENT, UNDERSTOOD IT, AND AGREE TO BE BOUND BY ITS TERMS AND CONDITIONS. YOU ALSO AGREE THAT THIS AGREEMENT IS THE COMPLETE AND EXCLUSIVE STATEMENT OF AGREEMENT BETWEEN YOU AND CANON CONCERNING THE SUBJECT MATTER HEREOF AND SUPERSEDES ALL PROPOSALS OR PRIOR AGREEMENTS, VERBAL OR WRITTEN, AND ANY OTHER COMMUNICATIONS BETWEEN YOU AND CANON RELATING TO THE SUBJECT MATTER HEREOF. NO AMENDMENT TO THIS AGREEMENT SHALL BE EFFECTIVE UNLESS SIGNED BY A DULY AUTHORISED REPRESENTATIVE OF CANON.
Should you have any questions concerning this Agreement, or if you desire to contact Canon for any reason, please write to Canon's sales subsidiary or distributor/dealer, serving the country where you obtained the Products.

This README file contains supplemental information to help you install and use your fax driver software with Microsoft Windows.
As with most software and hardware products, some information is made available after the development of the manual. Updated information regarding this driver software is provided in this README file. If you require additional assistance, please contact your local Canon company.
Windows and Windows Vista are either registered trademarks or trademarks of Microsoft Corporation in the United States and/or other countries.
Other product and company names herein may be the trademarks of their respective owners.
CONTENTS
Overview
System Requirements
Installing the Fax Driver
Accessing Help Information
Available Number of Destinations
Cautions, Limitations and Restrictions
Restrictions Regarding Device Settings
Overview
This fax driver allows you to send a fax from any Windows application to a remote fax machine if your machine contains an optional fax board.
System Requirements
The Canon Generic Fax Driver can be used in the following environments:
Operating System Software
Microsoft Windows XP
Microsoft Windows Vista
Microsoft Windows 7
Microsoft Windows 8
Microsoft Windows 8.1
Microsoft Windows Server 2003
Microsoft Windows Server 2008
Microsoft Windows Server 2008 R2 (64bit only)
Microsoft Windows Server 2012 (64bit only)
Microsoft Windows Server 2012 R2 (64bit only)
With Server-Based Computing Environment
Compatible Windows Terminal Server (Service)
Microsoft Windows Server 2003
Microsoft Windows Server 2008
Microsoft Windows Server 2008 R2 (64bit only)
Microsoft Windows Server 2012 (64bit only)
Microsoft Windows Server 2012 R2 (64bit only)
Compatible Software
Citrix Presentation Server 4.5
Citrix XenApp 5.0
Citrix XenApp 6.0 (64bit only)
Citrix XenApp 6.5 (64bit only)
Citrix XenDesktop 4.0
Citrix XenDesktop 5.0
Citrix XenDesktop 5.5
Citrix XenDesktop 5.6
Citrix XenDesktop 7.0
Computer
Any computer which runs the above operating system software properly.
However, at least one of the following output ports is required:
parallel printer port (LPT1, LPT2, etc.)
USB port
network interface
Installing the Fax Driver
To use this fax driver with software applications that operate with Microsoft Windows, use the following installation procedure.

NOTE
If you use a SMB (NetBIOS network) printer as a shared printer on the server computer, use the Add Printer Wizard, and select "Network printer" when installing the fax driver. Before installation, log into Windows as an Administrator. If a message prompting you to restart your computer is displayed when using the installer, make sure to restart your computer. If you do not restart your computer, existing drivers may not operate correctly.
If you are using the printer auto-creation mechanism in a Citrix XenApp (Presentation Server) environment, you may not be able to correctly install this driver using the Installer. If so, restart the XenApp Server computer and check the Printers folder ([Printers and Faxes] folder in Windows Server 2003). If any existing printer icons are no longer displayed, re-install the relevant fax drivers in the XenApp Server computer using the Add Printer Wizard in the Printers folder.
Then, before starting the Installer to install this driver, disconnect all client printers from all the ICA sessions using the ICA Client Printer Configuration utility. After installing the driver, restart the ICA Client Printer Configuration utility and reconnect the printers.

To discover a fax on a network automatically:
If you are using a TCP/IP network environment, refer to the following procedure. You can easily install the driver by selecting the fax from a list of faxes automatically discovered on the TCP/IP network.
* If you do not know what network environment (network protocol) you are using, check with your network supervisor.
1. Double-click the [Setup.exe] icon to start the installer.
* Depending on the environment you are using the [Setup.exe] icon may be displayed as [Setup].
2. The wizard is displayed, and the user license agreement is displayed on the screen. Confirm the content of the license agreement and click [Yes].
* If Canon Driver Information Assist Service is already installed and you are using an operating system equipped with Windows Firewall, a message which asks if you want to change the Windows Firewall setting is displayed during the installation.
If you select [Yes], Windows Firewall will be configured to unblock the connection for Canon Driver Information Assist Service, so that you can set up the printer configuration automatically or use the Department ID Management feature.
If you select [No], you cannot use Canon Driver Information Assist Service.
3. Select [Standard], then click [Next].
4. Select the process to execute, then click [Next].
If you want to get device information and use the department ID management function in a shared printer environment, when installing the driver on the print server, select the [Canon Driver Information Assist Service] check box in the process selection screen.
* If you are using an operating system equipped with Windows Firewall, a message which asks if you want to change the Windows Firewall setting is displayed during the installation.
If you select [Yes], Windows Firewall will be configured to unblock the connection for Canon Driver Information Assist Service, so that you can set up the printer configuration automatically or use the Department ID Management feature.
If you select [No], you cannot use Canon Driver Information Assist Service.
* If you are installing this driver for the first time, proceed to the next step.
5. Select the fax to install from [Fax List], then click [Next].
* If you want to use a customized fax name or install the driver as the default driver, select [Set Fax Information] and configure the fax information settings.
6. Confirm the installation settings, and click [Start]. The installation will begin.
7. When the installation completion screen is displayed, click [Exit].
The installation procedure is complete.
To install using a USB connection:
1. Turn off the device.
2. Start the Installer → follow the instructions in the dialog boxes.
For details, see steps 1 to 2 of "To discover a fax on a network automatically."
3. Select [USB Connection], and then click the [Next] button.
4. Click the [Yes] button in the message box asking if you want to start the installation.
5. When a dialog box prompts, connect the USB plug, and then turn the printer on.
* If installation fails in this screen, try performing the following procedure.
- If the Device Is Not Recognized When Connected by USB
6. After the files are copied, click the [Exit] button to finish the installation program.
If the Device Is Not Recognized When Connected by USB
If the device is not recognized when connected by USB, try performing the following procedure.
1. Connect the printer and computer with a USB cable, then turn the printer on.
2. Display the Device Manager.
Windows XP: Right-click [My Computer] - select [Administration] - [Device Manager]
Windows Vista: Select [Control Panel] - [System and Maintenance] - [Device Manager]
Windows 7/Server 2008 R2: Select [Control Panel] - [Hardware and Sound] - [Device Manager]
Windows 8/8.1/Server 2012/2012 R2: From the desktop, display the charm bar to the right of the screen, and click or tap [Settings] - [Control Panel] - [Device Manager].
3. In [Other Devices], right-click the name of the printer you are using → execute [Delete].
The printer name becomes
"Canon + <model name>"
When the above procedure is finished, reinstall the driver.
To set the port manually:
1. Double-click the [Setup.exe] icon to start the installer.
* Depending on the environment you are using the [Setup.exe] icon may be displayed as [Setup].
2. The wizard is displayed, and the user license agreement is displayed on the screen. Confirm the content of the license agreement and click [Yes].
* If Canon Driver Information Assist Service is already installed and you are using an operating system equipped with Windows Firewall, a message which asks if you want to change the Windows Firewall setting is displayed during the installation.
If you select [Yes], Windows Firewall will be configured to unblock the connection for Canon Driver Information Assist Service, so that you can set up the printer configuration automatically or use the Department ID Management feature.
If you select [No], you cannot use Canon Driver Information Assist Service.
3. Select [Custom], then click [Next].
4. Select the process to execute, then click [Next].
If you want to get device information and use the department ID management function in a shared printer environment, when installing the driver on the print server, select the [Canon Driver Information Assist Service] check box in the process selection screen.
* If Canon Driver Information Assist Service is already installed and you are using an operating system equipped with Windows Firewall, a message which asks if you want to change the Windows Firewall setting is displayed during the installation.
If you select [Yes], Windows Firewall will be configured to unblock the connection for Canon Driver Information Assist Service, so that you can set up the printer configuration automatically or use the Department ID Management feature.
If you select [No], you cannot use Canon Driver Information Assist Service.
* If you are installing this driver for the first time, proceed to the next step.
5. Select the port that the fax is connected to from the [Port] drop-down list or [Add Port], then click [OK]. Set the port in the displayed dialog box.
Standard port: Select this if you are using LPT or a pre-set LPR port.
Network: Select this if you are using a fax that is set to be shared on a network.
Add port: Select this if you want to add and use a new LPR port etc.
6. Enter a fax name in [Fax Name], then click [Next].
* If you are installing the driver as the default driver, select [Set as Default].
7. Confirm the installation settings, and click [Start]. The installation will begin.
8. When the installation completion screen is displayed, click [Exit].
The installation procedure is complete.
To install using the Add Printer Wizard:
1. Click the Start button, point to Settings, and then click Printers.
If you are using Windows XP Professional/Server 2003, on the [Start] menu, click [Printers and Faxes].
If you are using Windows XP Home Edition, on the [Start] menu, click [Control Panel], [Printers and Other Hardware], and then [Printers and Faxes].
If you are using Windows Vista/Server 2008, on the [Start] menu, click [Control Panel], and then [Printers]
If you are using Windows 7/Server 2008 R2, on the [Start] menu, click [Devices and Printers].
If you are using Windows 8/8.1/Server 2012/2012 R2, from the desktop, display the charm bar to the right of the screen, and click or tap [Settings] - [Control Panel] - [Devices and Printers].
2. In the Printers folder, double-click the [Add Printer] icon (Windows XP/Server 2003) or click [Add a printer] (Windows Vista/7/8/8.1/Server 2008/2008 R2/2012/2012 R2) to start the Add Printer Wizard.
3. Confirm the Wizard is started, and then click the [Next] button.
4. Follow the instructions on the screen to continue with the installation.
5. Click the [Have Disk] button.
6. Click the [Browse] button to select the ".inf" file, and then click the [OK] button.
\FAX\us_eng\32BIT\Driver
\FAX\us_eng\x64\Driver
* The path may differ from those described above, depending on the driver you are using.
7. Select your fax model from Printers, and then click the [Next] button.
8. Follow the instructions on the screen to continue, and then click the [Finish] button to start copying the files.
You are now ready to send a fax from any Windows software application.
Accessing Help Information
You can locate additional help for questions you may have regarding your fax in the Online Help file provided with the driver. In the fax properties dialog box, you can click [Help] to display additional information about every feature and option in the fax driver.
Available Number of Destinations
The number of destinations you are able to send to at one time varies according to the following settings.
(1) When [Set the number of destinations that can be specified at once to 2000] is selected:
If [Cover Sheet Attachment] is [None]: 2000
If [Cover Sheet Attachment] is [Different Sheet to Each Destination]: 100
If [Cover Sheet Attachment] is [Same Sheet to All Destinations]: 2000
(2) When [Set the number of destinations that can be specified at once to 2000] is deselected:
If [Cover Sheet Attachment] is [None]: 500
If [Cover Sheet Attachment] is [Different Sheet to Each Destination]: 100
If [Cover Sheet Attachment] is [Same Sheet to All Destinations]: 500

NOTE
In the case of groups, the above number of destinations is the number of personal destinations registered in the group. The specified number of destinations (among the above) is sent separated into multiple jobs. Consequently, in the job printing log list etc., they may be displayed as separate fax transmission files.
There is a limit to the number of fax job destinations that can be retained in the device. In some printer models, after a fax job is sent, if the number of destinations exceeds the limit, the last job(s) sent may be deleted. If destinations exceeding the limit of the group are registered, be careful that the fax is not sent continuously to multiple group destinations.

Cautions, Limitations and Restrictions
Do not specify more than 1 for the Copies option in the application since the fax may be sent more than once in some applications when the [Copies] option is specified in the application.
If double quotation marks or CSV separators are included in any of the items (Such as name and fax numbers) stored in a CSV file, the addresses stored in the file may not be imported to the address book correctly.
If you have upgraded your operating system from Windows XP/Server 2003 to Windows Vista, you will no longer be able to access the address book. If this is the case, perform the following procedure.
(1) Copy the address book files (gpfax.adr and gpfax.idx) from the system folder (the default system folder is "C:\Windows") to another folder (e.g. "My Documents"). This step can be carried out before or after you upgrade the system.
(2) After you have upgraded the system, reinstall the fax driver in the new system, open the [Edit Address Book] sheet, click the [Specify a folder] button, and choose the folder you copied the address book files to in step 1 (e.g. "My Documents") as the address book folder.
(3) Click the [Yes] button in the following dialog box.
If double quotation marks are included in any of the items (Such as names and fax numbers) stored in an ABK file (*.abk), the addresses stored in the file may not be imported to the address book correctly.
When you log on to an Administrator account that is different from the one used to install the software, you will not be able to access the driver properties with Administrator privileges. To access the driver properties, select [Run as Administrator].
In a 64-bit environment, the address book cannot be used with certain applications. If you are using an application that cannot utilize the address book, convert the address book to a CSV file, then import the CSV file into the fax driver as an address book.
For Windows Server 2008 installed with Server Core option, the following limitations exist on using the fax driver.
You cannot install the driver with the installer. Use the installation options of Windows.
Some fax options are not available under local environment or Windows Remote Desktop environment.
If you forget the password you have set for [Protect with Password when Exporting Address List] in the [Security Settings] dialog box of the [Special] sheet, you will not be able to export the address list. You can still perform operations other than exporting (browsing, adding, editing, deleting, etc.). If you want to export an address list, you will have to recreate the address list you want to export.
You cannot use the following address books with driver versions earlier than version 8.70:
Address books that have been newly created in version 8.70 or later drivers.
Address books that were created in older versions and imported into version 8.70 or later drivers.
However, you can use address books exported to files in driver versions earlier than version 8.70.
If you are using a printer (AutoCreatedPrinter) created with the "Auto Created Client Printer" function of Citrix XenDesktop, you may not be able to use the Department ID Management function or the Get Device Status function.
If this is the case, use the Citrix XenDesktop Universal Printer Driver (UPD), or select a Standard TCP/IP Port for which the IP address of a printer you are actually outputting to have been set.
"Mobile Address Book" may display in Messaging API address book. But the address book contacts will not be listed because the address book does not have fax related information.
If both a printer driver (or fax driver) and a USB-compliant scanner driver are not installed, a device connected by USB is recognized as new hardware, and although the following may occur, driver operations will not be affected.
Windows XP/Vista: A dialog box appears each time you connect the device by USB.
Windows 7/8/8.1: A warning icon is displayed on the corresponding printer icon in the [Devices and Printers] folder.
The driver is still operable in these states. To avoid these phenomenons, install the USB-compliant scanner driver (Color Network ScanGear 2 USB). For instructions on how to install the scanner driver, see the readme file provided with the driver.
Select [Store Sent Fax Information and Image] and the sent image will be stored only on the fax driver. The sent image and send results may not be the same as those on your machine. To check the send results of a sent fax, check the communication logs on your machine.
The communication mode you select when using IP-Fax should match the communication environment of the device. If you do not select the appropriate communication mode, it will lead to incorrect transmissions and send errors.
If you are using a device made for Korea, the USA, or Canada, if you enter more than 40 single-byte numeric characters for the fax number, an error will occur at the device and the fax will not be sent.
If you send using a paper size other than A4, depending on the application, you might not be able to send using the specified paper size. If this happens, reduce the magnification of the original data, specify A4, and resend the fax.
Depending on the application, if the number of destinations in the address book list is large, it might not operate correctly.
Fax images saved with this driver cannot be read by fax drivers prior to version 9.xx.
Profiles created with this driver cannot be used with fax drivers prior to version 9.xx.
When exporting Canon Address Book files (*.abk), you can specify the character code. When importing Canon Address Book files (*.abk), there are some printer models that cannot import a Canon Address Book file (*.abk) unless the character code of the imported file matches a character code supported by the device.
In this driver, only devices supported by fax drivers of version 9.00 or earlier support USB installation.
Before installing this driver, correctly configure the [Control Panel] - [Region and Language] settings. If the correct region is not set, the fax driver may not operate correctly.
This driver can coexist with a version 9.xx or earlier fax driver.
This driver cannot be used to update a version 9.xx or earlier fax driver.
If SNMP is not set at the device, you may not be able to install the driver using [Standard].
Restrictions Regarding Device Settings
With this fax driver, if you use printer model-dependent functions, you must get the device information and set beforehand the options that are installed from [Device Settings] – [Get Device Status].
If you cannot get the device information from [Device Settings] – [Get Device Status] (for example, if you are connected via USB), to use the functions corresponding to the printer model you are using, set the attached options manually in the [Device Settings] sheet.
Take care that you do not set functions with the fax driver that are not in the printer model as this can lead to mis-transmissions and transmission errors.
If you set a sender with a printer model that does not have the specify sender function, you will not be able to use that function.
If you select a fax board that is not compatible with the printer model you are using, and select a line that does not match a valid line to send from, there is a possibility that the fax will be sent via a different line.
If you attempt to send with settings that do not match the printer model you are using for the subaddress authentication mode, department ID management authentication mode, and IP fax communication mode, you will not be able to send.
If you specify the send time with a printer model that does not have the send time function, you cannot use that function.
If you specify the subaddress function with a printer model that does not have the subaddress function, you cannot use that function.
If you specify the [Set the number of destinations that can be specified at once to 2000] function and attempt to send with a printer model that does not support that function, this will result in a communication error or transmission error.
If you set department ID management with a printer model that does not have the department ID management function, you cannot use that function.

Copyright Canon Inc. 1999