Berger Samba 6oz Polyester is a hybrid fabric useable for both UV-cured and dye-sublimation inks.  The material is typically manufactured with the dye-sublimation side wound out.  The inside-wound side has a grippy top coat to hold UV ink.  Loading such a roll as print-side-out on the Colorado M-Series faces the top coat toward the metal panels along the media path.  The high resistance will cause the media to snag.

Unless the packaging specifically says otherwise, the roll should be loaded as print-side-in from drawer Position 2.  Use a semi-rigid leader material to help get it to the platen and an unlocked tension bar.  Refer to the Operations Guide for that procedure.